RS232 Bricklet – Tinkerforge

- Getting Started
- Hardware
- Software
- Starter Kits
- Embedded Boards
- Specifications

# RS232 Bricklet

Note

This Bricklet is currently work-in-progress!

## Features

- Can send and receive serial data
- Provides RS232 and UART-TTL interface
- Configurable baudrate, parity, stop bits, word length and flow control

## Description

The RS232 Bricklet can be used to extend the features of Bricks by the capability to send and receive RS232 data.

## Technical Specifications

Property | Value
--- | ---
Current Consumption | TBDmA
Baudrate | 300 - 230400baud
Parity | None / Odd / Even / Forced Parity 1 / Forced Parity 0
Stop bits | 1 / 2
Word length | 5 / 6 / 7 / 8
Flow control | Software / Hardware / Off
Dimensions (W x D x H) | 45 x 35 x 15mm (1.77 x 1.38 x 0.59")
Weight | TBDg

## Resources

- Schematic (Download)
- Outline and drilling plan (Download)
- Source code and design files (Download)

## Test your RS232 Bricklet

## Case

## Programming Interface

See Programming Interface for a detailed description.

Language | API | Examples | Installation
--- | --- | --- | ---
Modbus | API |  |
TCP/IP | API |  |
C/C++ | API | Examples | Installation
C# | API | Examples | Installation
Delphi/Lazarus | API | Examples | Installation
Java | API | Examples | Installation
JavaScript | API | Examples | Installation
LabVIEW | API | Examples | Installation
Mathematica | API | Examples | Installation
MATLAB/Octave | API | Examples | Installation
Perl | API | Examples | Installation
PHP | API | Examples | Installation
Python | API | Examples | Installation
Ruby | API | Examples | Installation
Shell | API | Examples | Installation
Visual Basic .NET | API | Examples | Installation

The content of this page is licensed under Creative Commons Attribution 3.0 Unported License.