Industrial Analog Out Bricklet – Tinkerforge

- Getting Started
- Hardware
- Software
- Starter Kits
- Embedded Boards
- Specifications

# Industrial Analog Out Bricklet

Note

This Bricklet is currently work-in-progress!

## Features

- Simultaneous programmable voltage and current output
- Outputs voltage between 0V and 10V
- Outputs current between 0mA and 24mA
- No external supply necessary

## Description

The Industrial Analog Out Bricklet can be used to extend the features of Bricks by the capability to output voltage and current.

Voltage and current output are simultaneous. The voltage can be given in mV and the current in µV.

## Technical Specifications

Property | Value
--- | ---
DAC | DAC7760
Current Consumption | TBDmA
Resolution | up to 1.2mV / 4.8µA

Voltage Ranges

- 0V - 5V
- 0V - 10V

Current Ranges

- 4mA - 20mA
- 0mA - 20mA
- 0mA - 24mA

Dimensions (W x D x H) | 40 x 40 x 11mm (1.57 x 1.57 x 0.43")
Weight | TBDg

## Resources

- DAC7760 Datasheet (Download)
- Schematic (Download)
- Outline and drilling plan (Download)
- Source code and design files (Download)

## Test your Industrial Analog Out Bricklet

## Case

## Programming Interface

See Programming Interface for a detailed description.

Language | API | Examples | Installation
--- | --- | --- | ---
Modbus | API |  |
TCP/IP | API |  |
C/C++ | API | Examples | Installation
C# | API | Examples | Installation
Delphi/Lazarus | API | Examples | Installation
Java | API | Examples | Installation
JavaScript | API | Examples | Installation
LabVIEW | API | Examples | Installation
Mathematica | API | Examples | Installation
MATLAB/Octave | API | Examples | Installation
Perl | API | Examples | Installation
PHP | API | Examples | Installation
Python | API | Examples | Installation
Ruby | API | Examples | Installation
Shell | API | Examples | Installation
Visual Basic .NET | API | Examples | Installation

The content of this page is licensed under Creative Commons Attribution 3.0 Unported License.