Construction - RED Brick Weather Station – Tinkerforge

- Getting Started
  - Primer
  - Tutorials
  - FAQ
- Hardware
  - Bricks
  - Bricklets
  - Master Extensions
  - Power Supplies
  - Accessories
  - Timeline
- Software
  - Brick Daemon (brickd)
  - Brick Viewer (brickv)
  - API Bindings
  - Firmwares and Plugins
  - Device Identifier
  - Source Code and Bug Tracking
  - Programming Interface
- Starter Kits
  - Weather Station
    - Features
    - Description
    - Technical Specifications
    - Resources
    - Firmware updating and first tests
    - Demo Application
    - Construction
      - Basic
      - With Wi-Fi
      - With RED Brick
        - Stack on Backside
      - With Raspberry Pi
    - Projects
    - Further Enhancements
  - Hardware Hacking
  - Server Room Monitoring
  - Blinkenlights
  - Internet of Things
  - Camera Slider
- Embedded Boards
  - Raspberry Pi
- Specifications
  - Technical Data
  - TCP/IP Protocol
  - Modbus Protocol
  - Wireshark Dissector

# Construction - RED Brick Weather Station

It is possible to control the Weather Station without any external (Embedded-) PC by using a RED Brick mounted into the case. In this tutorial we well use a USB Power Supply to power the stack. It is also possible to power the stack with a Step-Down Power Supply together with a DC Jack Adapter to power the stack. For details about this see the Wi-Fi Weather Station construction section.

The RED Brick Weather Station is an extension of the basic version. You should build the basic version first and then modify it as described down below.

## Stack on Backside

Just mount the stack consisting of RED Brick and Master Brick to the back side of the case.

We can now mount the front of the case to the back again.

The content of this page is licensed under Creative Commons Attribution 3.0 Unported License.