Analog In Bricklet 2.0 – Tinkerforge

- Getting Started
- Hardware
- Software
- Starter Kits
- Embedded Boards
- Specifications

# Analog In Bricklet 2.0

Note

This Bricklet is currently work-in-progress!

## Features

- Measures voltages up to 42V (DC)
- Full-scale resolution of 10mV

## Description

The Analog In Bricklet 2.0 can be used to extend the features of Bricks by the capability to measure voltages. The voltage can be read out in Volt directly without conversions necessary.

With configurable events it is possible to react on changing voltages without polling.

## Technical Specifications

Property | Value
--- | ---
Current Consumption | TBDmA
Voltage | 0V - 42V (DC), 12bit resolution ( 10mV)
Dimensions (W x D x H) | 35 x 30 x 14mm (1.38 x 1.18 x 0.55")
Weight | TBDg

## Resources

- Schematic (Download)
- Outline and drilling plan (Download)
- Source code and design files (Download)

## Test your Analog In Bricklet 2.0

## Case

## Programming Interface

See Programming Interface for a detailed description.

Language | API | Examples | Installation
--- | --- | --- | ---
Modbus | API |  |
TCP/IP | API |  |
C/C++ | API | Examples | Installation
C# | API | Examples | Installation
Delphi/Lazarus | API | Examples | Installation
Java | API | Examples | Installation
JavaScript | API | Examples | Installation
LabVIEW | API | Examples | Installation
Mathematica | API | Examples | Installation
MATLAB/Octave | API | Examples | Installation
Perl | API | Examples | Installation
PHP | API | Examples | Installation
Python | API | Examples | Installation
Ruby | API | Examples | Installation
Shell | API | Examples | Installation
Visual Basic .NET | API | Examples | Installation

The content of this page is licensed under Creative Commons Attribution 3.0 Unported License.