Industrial Dual Analog In Bricklet – Tinkerforge

- Getting Started
- Hardware
- Software
- Starter Kits
- Embedded Boards
- Specifications

# Industrial Dual Analog In Bricklet

Note

This Bricklet is currently work-in-progress!

## Features

- Independently measures two voltages between -45V and 45V
- 24 bit resolution
- Calibrated to calibration standard at room temperature
- Full-scale accuracy of 0.1% / ±4mV
- Up to 976 samples per second

## Description

The Industrial Dual Analog In Bricklet can be used to extend the features of Bricks by the capability to measure voltages. Both channels of the Bricklet are calibrated. The voltage measurement can used with an extremely high level of confidence.

With configurable events it is possible to react on changing voltages without polling.

## Technical Specifications

Property | Value
--- | ---
ADC | MCP3911
Current Consumption | TBDmA
Channels | 2
Measurement Range | -45V - 45V
Resolution | 24bit resolution
Accuracy | 0.1% / ±4mV full scale
Dimensions (W x D x H) | 40 x 40 x 11mm (1.57 x 1.57 x 0.43")
Weight | TBDg

## Resources

- MCP3911 Datasheet (Download)
- Schematic (Download)
- Outline and drilling plan (Download)
- Source code and design files (Download)

## Test your Industrial Dual Analog In Bricklet

## Case

## Programming Interface

See Programming Interface for a detailed description.

Language | API | Examples | Installation
--- | --- | --- | ---
Modbus | API |  |
TCP/IP | API |  |
C/C++ | API | Examples | Installation
C# | API | Examples | Installation
Delphi/Lazarus | API | Examples | Installation
Java | API | Examples | Installation
JavaScript | API | Examples | Installation
LabVIEW | API | Examples | Installation
Mathematica | API | Examples | Installation
MATLAB/Octave | API | Examples | Installation
Perl | API | Examples | Installation
PHP | API | Examples | Installation
Python | API | Examples | Installation
Ruby | API | Examples | Installation
Shell | API | Examples | Installation
Visual Basic .NET | API | Examples | Installation

The content of this page is licensed under Creative Commons Attribution 3.0 Unported License.